5.02.69 - Release Notes (MD2_5.02.69_DIAGNOSTIC_2013-08-23)


      ECU data:
        * Support for ADM3, DiagV. 211 with software 11.01a
        * Support for ADM2 (204) and ADM3 (206 - 211) parameters 11/08 "Boost Thres. active" and 11/10 "Boost Thres Ramp"
        * Routine for ADM2 (204) and ADM3 (206 - 211) "Torque Threshold" deaktivated!
        * SCR commissioning routine without password protection (routine now listet in routines not anymore password routines!)
        * Bugfix:
           - no

      Software:
        * Bugfix:
           - SCR commissioning routine without password protection is working now



5.02.67 - Release Notes (MD2_5.02.67_DIAGNOSTIC_2013-01-15)  ATTENTION!!!! This version is locked - SCR routine not working!!!


      ECU data:
        * Support for FLA-CAN (DiagV. 6)
        * SCR commissioning routine without password protection
        * Bugfix:
           - no

      Software:
        * Bugfix:
           - no
          


5.02.67 - Release Notes (MD2_5.02.67_DIAGNOSTIC_2012-10-23)


      ECU data:
        * Support for MR2-B-SW24 (DiagV. 57)
        * Conversion tables added until SW23/24 (MR2)
        * Bugfix:
           - MR-CNG, DiagV. 105 (communication error at routines with required engine type information)
           - MR-CNG, all (improved fault code text and other)

      Software:
        * Bugfix:
           - CPC1, ID-Code now 00ffffff for XT/XN routines analog ADM3
           - CPC1, 7f/78 and FDOK-handling for KWP on J1939 implemented (GM diagnosis, parameter sets)
          


5.02.64 - Release Notes (MD2_5.02.64_DIAGNOSTIC_2011-10-10)


      ECU data:
        * Support for MR2-A-SW23 (DiagV. 56) and INS DiagV.60
        * Import file for CPC1 parameter group SCR for Boschung-AdBluetank (VDODIAG.PAR)

      Software:
        * Flash-Support for MR2-A/B with hardware 2.x
        * Bugfix:
           - USB/Peak-CAN driver
           - Import VDODIAG.PAR files for CPC1 (DiagV. 45, 46, 56)



5.02.61 - Release Notes


      ECU data:
        * Support for Tier4i (ADM DiagV. 210, CPC1 release 26 (DiagV. 56) and MR2-B-SW V23)
        * Import files for CPC1 parameter group SCR for MB-AdBluetanks (VDODIAG.PAR)
        * SCR commissioning routine with password protection (request of development
          department)




5.02.60 - Release Notes

      ECU data:
        * Support for ADM3 with SW90x and DiagV. 209 added (selective power ratings,
          control lever MBR and CC, improved J1939 data and error codes for MR2-B V22)
        * Default values improved
        * Conversion tables added and improved
        * Description data improved
        * New routines (e.g. read/write VIN , read CAL-ID (software calibration number)
          for MR2-B)
        * SCR commissioning and VIN writing routine without password protection
        * EHM expanded


          2010-08-23:
        * MR2-B (33, 35, 37), improved text display for "fan type"



      Software:
        * Safety concept improved
          - second password routine counter added
          - BM (Baumuster) positiv list for password routines
          - v-signal settings of ADMx parameter 8/2(1) with password protection, only
            1= "C3 from tachograph" and 5="J1939 TCO Shaft Speed and Vehicle Speed"
            without password
          - protection for old CPC1 parameter sets
        * ECU search list improved
        * Gateway functions for INS and ADMx improved
        * Import function for CPC1 parameter groups like SCR (VDODIAG.PAR)
        * 64-Bit OS support for Peak-CAN-USB


          2010-08-12:
        * Bugfix: "Click the language button before opening the parameter assistant and
                  parameter files"
                  (Error: MA02_32.EX_ => If you starting first time on PC without using
                  language button)
        * Bugfix: Transparent stripe on start of minidiag2 Assistant


          2010-08-23:
        * Safety concept
            - v-signal settings of ADMx parameter 8/2(1) with password protection, only
              0= "none", 1= "C3 from tachograph" and 5="J1939 TCO Shaft Speed and Vehicle
              Speed" without password
        * Update of "Manual - New Software Functions.pdf"









