MATERIAL SAFETY DATA SHEET

SECTION 1	 PRODUCT AND COMPANY IDENTIFICATION	

PRODUCT
Product Name:    MOBIL DELVAC 1300 SUPER 15W-40
Product Description:   Base Oil and Additives
Product Code:     440693-00,   970529
Intended Use:    Engine oil

COMPANY IDENTIFICATION
Supplier:		EXXON MOBIL CORPORATION 
 3225 GALLOWS RD. 
FAIRFAX, VA.  22037     USA
 24 Hour Health Emergency	 609-737-4411	
 Transportation Emergency Phone	 800-424-9300	
 ExxonMobil Transportation No.	 281-834-3296	
 MSDS Requests	 713-613-3661	
 Product Technical Information	 800-662-4525, 800-947-9147	
 MSDS Internet Address	 http://www.exxon.com, http://www.mobil.com	

 SECTION 2	 COMPOSITION / INFORMATION ON INGREDIENTS	
 
No Reportable Hazardous Substance(s) or Complex Substance(s).     

SECTION 3	 HAZARDS IDENTIFICATION	
 
This material is not considered to be hazardous according to regulatory guidelines (see (M)SDS Section 15).

POTENTIAL HEALTH EFFECTS
 Low order of toxicity.  Excessive exposure may result in eye, skin, or respiratory irritation.  High-pressure injection under skin may cause serious damage. 

 NFPA Hazard ID: 	Health:    0	Flammability:   1	Reactivity:   0	
 HMIS Hazard ID: 	Health:    0	Flammability:   1	Reactivity:   0	

NOTE:   This material should not be used for any other purpose than the intended use in Section 1 without expert advice. Health studies have shown that chemical exposure may cause potential human health risks which may vary from person to person.  

 SECTION 4	FIRST AID MEASURES	

INHALATION
Remove from further exposure.  For those providing assistance, avoid exposure to yourself or others.  Use adequate respiratory protection.  If respiratory irritation, dizziness, nausea, or unconsciousness occurs, seek immediate medical assistance.  If breathing has stopped, assist ventilation with a mechanical device or use mouth-to-mouth resuscitation.

SKIN CONTACT
Wash contact areas with soap and water.  If product is injected into or under the skin, or into any part of the body, regardless of the appearance of the wound or its size, the individual should be evaluated immediately by a physician as a surgical emergency. Even though initial symptoms from high pressure injection may be minimal or absent, early surgical treatment within the first few hours may significantly reduce the ultimate extent of injury.

EYE CONTACT
Flush thoroughly with water.  If irritation occurs, get medical assistance.

INGESTION
First aid is normally not required. Seek medical attention if discomfort occurs.

SECTION 5	FIRE FIGHTING MEASURES	

EXTINGUISHING MEDIA
Appropriate Extinguishing Media:  Use water fog, foam, dry chemical or carbon dioxide (CO2) to extinguish flames.

Inappropriate Extinguishing Media:  Straight Streams of Water 

FIRE FIGHTING
Fire Fighting Instructions:  Evacuate area.  Prevent runoff from fire control or dilution from entering streams, sewers, or drinking water supply.  Firefighters should use standard protective equipment and in enclosed spaces, self-contained breathing apparatus (SCBA).  Use water spray to cool fire exposed surfaces and to protect personnel.  

Hazardous Combustion Products:   Aldehydes, Sulfur oxides, Oxides of carbon, Incomplete combustion products, Smoke, Fume

FLAMMABILITY PROPERTIES 
Flash Point [Method]:  >215C  (419F) [ ASTM D-92]
Flammable Limits (Approximate volume % in air):   LEL:  0.9     UEL: 7.0
Autoignition Temperature:  N/D 

 SECTION 6	ACCIDENTAL RELEASE MEASURES	

NOTIFICATION PROCEDURES
In the event of a spill or accidental release, notify relevant authorities in accordance with all applicable regulations. U.S. regulations require reporting releases of this material to the environment which exceed the reportable quantity or oil spills which could reach any waterway including intermittent dry creeks.  The National Response Center can be reached at (800)424-8802.

SPILL MANAGEMENT
Land Spill:  Stop leak if you can do it without risk.  Recover by pumping or with suitable absorbent.

Water Spill:  Stop leak if you can do it without risk.  Confine the spill immediately with booms.   Warn other shipping.   Remove from the surface by skimming or with suitable absorbents.   Seek the advice of a specialist before using dispersants.

Water spill and land spill recommendations are based on the most likely spill scenario for this material; however, geographic conditions, wind, temperature, (and in the case of a water spill) wave and current direction and speed may greatly influence the appropriate action to be taken.  For this reason, local experts should be consulted.  Note:  Local regulations may prescribe or limit action to be taken. 

ENVIRONMENTAL PRECAUTIONS
Large Spills:  Dike far ahead of liquid spill for later recovery and disposal.  Prevent entry into waterways, sewers, basements or confined areas.

 SECTION 7	HANDLING AND STORAGE	

HANDLING
Avoid contact with used product. Prevent small spills and leakage to avoid slip hazard.       

Static Accumulator:   This material is a static accumulator.

STORAGE
Do not store in open or unlabelled containers.           

 SECTION 8	EXPOSURE CONTROLS / PERSONAL PROTECTION	

 
Exposure limits/standards for materials that can be formed when handling this product:   When mists / aerosols can occur, the following are recommended:  5 mg/m³ - ACGIH TLV,  10 mg/m³ - ACGIH STEL, 5 mg/m³ - OSHA PEL.  

NOTE: Limits/standards shown for guidance only.  Follow applicable regulations.

ENGINEERING CONTROLS

The level of protection and types of controls necessary will vary depending upon potential exposure conditions.  Control measures to consider:
 No special requirements under ordinary conditions of use and with adequate ventilation. 

PERSONAL PROTECTION
 
Personal protective equipment selections vary based on potential exposure conditions such as applications, handling practices, concentration and ventilation.  Information on the selection of protective equipment for use with this material, as provided below, is based upon intended, normal usage.  

Respiratory Protection:   If engineering controls do not maintain airborne contaminant concentrations at a level which is adequate to protect worker health, an approved respirator may be appropriate.  Respirator selection, use, and maintenance must be in accordance with regulatory requirements, if applicable.  Types of respirators to be considered for this material include: 
 No special requirements under ordinary conditions of use and with adequate ventilation. 

For high airborne concentrations, use an approved supplied-air respirator, operated in positive pressure mode.  Supplied air respirators with an escape bottle may be appropriate when oxygen levels are inadequate, gas/vapor warning properties are poor, or if air purifying filter capacity/rating may be exceeded.

Hand Protection:   Any specific glove information provided is based on published literature and glove manufacturer data. Work conditions can greatly effect glove durability; inspect and replace worn or damaged gloves. The types of gloves to be considered for this material include: 
 No protection is ordinarily required under normal conditions of use.

Eye Protection:   If contact is likely, safety glasses with side shields are recommended.

Skin and Body Protection:    Any specific clothing information provided is based on published literature or manufacturer data.  The types of clothing to be considered for this material include:
 No skin protection is ordinarily required under normal conditions of use.  In accordance with good industrial hygiene practices, precautions should be taken to avoid skin contact.

Specific Hygiene Measures:   Always observe good personal hygiene measures, such as washing after handling the material and before eating, drinking, and/or smoking.  Routinely wash work clothing and protective equipment to remove contaminants.  Discard contaminated clothing and footwear that cannot be cleaned. Practice good housekeeping.

ENVIRONMENTAL CONTROLS
 See Sections  6,  7, 12, 13.

SECTION 9	 PHYSICAL AND CHEMICAL PROPERTIES	

Typical physical and chemical properties are given below.   Consult the Supplier in Section 1 for additional data.

GENERAL INFORMATION
Physical State:    Liquid 
Color:   Brown
Odor:   Characteristic
Odor Threshold:   N/D

IMPORTANT HEALTH, SAFETY, AND ENVIRONMENTAL INFORMATION
Relative Density (at 15 C ):    0.874   
Flash Point [Method]:     >215C  (419F) [ ASTM D-92]
Flammable Limits (Approximate volume % in air):   LEL:  0.9     UEL: 7.0  
Autoignition Temperature:  N/D 
Boiling Point / Range:    > 316C  (600F)
Vapor Density (Air = 1):   N/D
Vapor Pressure:   < 0.013 kPa (0.1 mm Hg) at 20 C
Evaporation Rate (n-butyl acetate = 1):   N/D
pH:   N/A
Log Pow (n-Octanol/Water Partition Coefficient):   > 3.5
Solubility in Water:   Negligible
Viscosity:   113 cSt  (113 mm2/sec ) at 40 C  |  15 cSt  (15 mm2/sec) at 100C
Oxidizing Properties:  See Sections 3, 15, 16.

OTHER INFORMATION
Freezing Point:   N/D
Melting Point:   N/A
Pour Point:      -27°C  (-17°F)   
DMSO Extract (mineral oil only), IP-346:    < 3 %wt 

 SECTION 10	 STABILITY AND REACTIVITY 	

STABILITY:  Material is stable under normal conditions.

CONDITIONS TO AVOID:  Excessive heat. High energy sources of ignition.

MATERIALS TO AVOID:   Strong oxidizers

HAZARDOUS DECOMPOSITION PRODUCTS:  Material does not decompose at ambient temperatures.

HAZARDOUS POLYMERIZATION:  Will not occur.

SECTION 11	 TOXICOLOGICAL INFORMATION	

ACUTE TOXICITY
 Route of Exposure	 Conclusion / Remarks	
Inhalation		
Toxicity (Rat): LC50 > 5000 mg/m3	Minimally Toxic. Based on test data for structurally similar materials.	
Irritation: No end point data.	Negligible hazard at ambient/normal handling temperatures. Based on assessment of the components.	
		
Ingestion		
Toxicity (Rat): LD50 > 2000 mg/kg	Minimally Toxic. Based on test data for structurally similar materials.	
		
Skin		
Toxicity (Rabbit): LD50 > 2000 mg/kg	Minimally Toxic. Based on test data for structurally similar materials.	
Irritation (Rabbit): Data available.	Negligible irritation to skin at ambient temperatures. Based on test data for structurally similar materials.	
		
Eye 		
Irritation (Rabbit): Data available.	May cause mild, short-lasting discomfort to eyes. Based on test data for structurally similar materials.	

CHRONIC/OTHER EFFECTS
             For the product itself:
 Diesel engine oils:  Not carcinogenic in animals tests.  Used and unused diesel engine oils did not produce any carcinogenic effects in chronic mouse skin painting studies.
Oils that are used in gasoline engines may become hazardous and display the following properties:  Carcinogenic in animal tests. Caused mutations in vitro. Possible allergen and photoallergen. Contains polycyclic aromatic compounds (PAC) from combustion products of gasoline and/or thermal degradation products.

Contains:
Base oil severely refined:  Not carcinogenic in animal studies. Representative material passes IP-346, Modified Ames test, and/or other screening tests. Dermal and inhalation studies showed minimal effects; lung non-specific infiltration of immune cells, oil deposition and minimal granuloma formation. Not sensitizing in test animals.

Additional information is available by request.
 
The following ingredients are cited on the lists below:  None.

--REGULATORY LISTS SEARCHED--	
 1 = NTP CARC	 3 = IARC 1	 5 = IARC 2B	
 2 = NTP SUS	 4 = IARC 2A	 6 = OSHA CARC	

 SECTION 12	 ECOLOGICAL INFORMATION	

The information given is based on data available for the material, the components of the material, and similar materials.

ECOTOXICITY   
             Material -- Not expected to be harmful to aquatic organisms. 

MOBILITY 
             Base oil component -- Low solubility and floats and is expected to migrate from water to the land.  Expected to partition to sediment and wastewater solids. 

PERSISTENCE AND DEGRADABILITY
Biodegradation: 
             Base oil component --  Expected to be inherently biodegradable   

BIOACCUMULATION POTENTIAL 
             Base oil component -- Has the potential to bioaccumulate, however metabolism or physical properties may reduce the bioconcentration or limit bioavailability.

    
 
 SECTION 13	 DISPOSAL CONSIDERATIONS	
 
Disposal recommendations based on material as supplied.  Disposal must be in accordance with current applicable laws and regulations, and material characteristics at time of disposal. 

DISPOSAL RECOMMENDATIONS
 Product is suitable for burning in an enclosed controlled burner for fuel value or disposal by supervised incineration at very high temperatures to prevent formation of undesirable combustion products. 
 
REGULATORY DISPOSAL INFORMATION
 RCRA Information: The unused product, in our opinion, is not specifically listed by the EPA as a hazardous waste (40 CFR, Part 261D), nor is it formulated to contain materials which are listed as hazardous wastes.  It does not exhibit the hazardous characteristics of ignitability, corrositivity or reactivity and is not formulated with contaminants as determined by the Toxicity Characteristic Leaching Procedure (TCLP).  However, used product may be regulated.

 Empty Container Warning PRECAUTIONARY LABEL TEXT:  Empty containers may retain residue and can be dangerous.  DO NOT PRESSURIZE, CUT, WELD, BRAZE, SOLDER, DRILL, GRIND OR EXPOSE SUCH CONTAINERS TO HEAT, FLAME, SPARKS, STATIC ELECTRICITY, OR OTHER SOURCES OF IGNITION; THEY MAY EXPLODE AND CAUSE INJURY OR DEATH.  Do not attempt to refill or clean container since residue is difficult to remove.  Empty drums should be completely drained, properly bunged and promptly returned to a drum reconditioner.  All containers should be disposed of in an environmentally safe manner and in accordance with governmental regulations.

 SECTION 14	 TRANSPORT INFORMATION	

LAND (DOT) :  Not Regulated for Land Transport
                   
LAND (TDG) :  Not Regulated for Land Transport

SEA (IMDG) :  Not Regulated for Sea Transport according to IMDG-Code

AIR (IATA) :  Not Regulated for Air Transport

 SECTION 15	 REGULATORY INFORMATION	

OSHA HAZARD COMMUNICATION STANDARD:   When used for its intended purposes, this material is not classified as hazardous in accordance with OSHA 29 CFR 1910.1200.

NATIONAL CHEMICAL INVENTORY LISTING:   TSCA
               Special Cases:
 
 Inventory	 Status	
 ELINCS	 Restrictions Apply	

EPCRA:  This material contains no extremely hazardous substances.

SARA (311/312) REPORTABLE HAZARD CATEGORIES:   None.

SARA (313) TOXIC RELEASE INVENTORY:  This material contains no chemicals subject to the supplier notification requirements of the SARA 313 Toxic Release Program.

The Following Ingredients are Cited on the Lists Below:  
Chemical Name	CAS Number	List Citations	
DIPHENYLAMINE	122-39-4	5, 9, 18	
PHOSPHORUS	7723-14-0	1, 4	
ZINC DITHIOPHOSPHATE	68649-42-3	15	

--REGULATORY LISTS SEARCHED--	
1 = ACGIH ALL	6 = TSCA 5a2	11 = CA P65 REPRO	16 = MN RTK	
 2 = ACGIH A1	7 = TSCA 5e	12 = CA RTK	17 = NJ RTK	
3 = ACGIH A2	8 = TSCA 6	13 = IL RTK	18 = PA RTK	
4 = OSHA Z	9 = TSCA 12b	14 = LA RTK	19 = RI RTK	
5 = TSCA 4	10 = CA P65 CARC	15 = MI 293		

Code key: CARC=Carcinogen; REPRO=Reproductive

 SECTION 16	OTHER INFORMATION	
N/D = Not determined, N/A = Not applicable

THIS SAFETY DATA SHEET CONTAINS THE FOLLOWING REVISIONS:
Revision Changes:
Section 05: Hazardous Combustion Products was modified.
Section 09: Viscosity was modified.
Section 09: Viscosity was modified.
Section 15: List Citations Table was modified.
Section 15: List Citation Table - Header was modified.
Section 15: SARA (313) TOXIC RELEASE INVENTORY - Header was modified.
Section 15: National Chemical Inventory Listing was modified.
Section 09: Relative Density was modified.
Section 16: MSN, MAT ID was modified.
Section 02: No components was modified.
Section 15: Special Cases - Header was added.
Section 15: Special Cases Table was added.
Section 15: Inventory - Header was added.
Section 15: Status - Header was added.
Section 02: Component table was deleted.
Section 15: SARA (313) TOXIC RELEASE INVENTORY - Table was deleted.
Section 15: SARA 313 - Chemical Name - Header was deleted.
Section 15: SARA 313 - CAS Number - Header was deleted.
Section 15: SARA313  - Typical Value - Header was deleted.
Section 02: Primary Ingredient Name was deleted.
Section 02: CAS Number was deleted.
Section 02: Concentration - Header was deleted.
Section 02: Substances Table - Header was deleted.
Section 02: Concentration Footnote was deleted.
Section 15:  TSCA Class 2 Statement was deleted.   
-----------------------------------------------------------------------------------------------------------------------------------------------------               
-----------------------------------------------------------------------------------------------------------------------------------------------------
The information and recommendations contained herein are, to the best of ExxonMobil's knowledge and belief, accurate and reliable as of the date issued.  You can contact ExxonMobil to insure that this document is the most current available from ExxonMobil.  The information and recommendations are offered for the user's consideration and examination.  It is the user's responsibility to satisfy itself that the product is suitable for the intended use.  If buyer repackages this product, it is the user's responsibility to insure proper health, safety and other necessary information is included with and/or on the container.  Appropriate warnings and safe-handling procedures should be provided to handlers and users.  Alteration of this document is strictly prohibited.  Except to the extent required by law, re-publication or retransmission of this document, in whole or in part, is not permitted.  The term, "ExxonMobil" is used for convenience, and may include any one or more of ExxonMobil Chemical Company, Exxon Mobil Corporation, or any affiliates in which they directly or indirectly hold any interest.

-----------------------------------------------------------------------------------------------------------------------------------------------------
 
Internal Use Only		
MHC:  0, 0, 0, 0, 0, 0	PPEC:   A	

 DGN:  2003305XUS  (1012124)
-----------------------------------------------------------------------------------------------------------------------------------------------------
Copyright 2002 Exxon Mobil Corporation, All rights reserved